|  |  |  |  |
| --- | --- | --- | --- |
| **1** | **1** | **Glasswasher Ecomax plus G403-11B** |  |
|  |  |  |  |

|  |  |  |  |
| --- | --- | --- | --- |
|  |  | **Total (Net)**  | **€** |
|  |  |  |  |

|  |  |
| --- | --- |
|  |  |
| Wash ware | According to DIN10512 section 7 |
| Rinse Type | One Tank Dishwasher |
| Design | Front door machine, adjustable as undercounter model |
| Heating | Electrical, 230 V/400 V-Connection |
| Capacity | Up to 40 Racks/h |
| Loading height | 315 mm |
|  |  |
|  |  |
|  |
| **Machine features**- Electronic control with temperature indication- Rotating top and bottom wash system to distribute the wash water evenly over the dishes- Negative stamped nozzles- Electric cable, flexible water supply hose and drain hose- Thermostop-function for guaranteed rinse temperatures- Integrated self-cleaning cycle |
| **PlusFeatures**- Deep-drawn wash tank- Improved energy efficiency- Double-walled housing and heat insulated front door- Tank strainer, coarse filter and pump suction casing- Door damping control- Fully equipped with detergent and rinse aid dispenser, rinse pressure pump and drain pump |
| **Rack equipment**1 Universal flat rack 400 x 400 mm, without sloped rows, plastic coated, height 115 mm 371450-83 |
| 1 Universal glass rack 400 x 400 mm, with 4 sloped rows à 90 mm, height 175 mm 371450-84 |

|  |
| --- |
|  |
| **Dimensions** |  |
| Machine housing width | 460 mm |
| Machine housing depth | 590 mm |
| Depth when door is open | 940 mm |
| Height | 705 mm |
| Loading height | 315 mm |
|  |  |
| **Capacity** |  |
| Cycle time P1/P2\* | 90 / 180 sec. |
| Capacity\*\* | Up to 40 Racks/h |
| Wash temperature | 55 °C |
| Rinse temperature | 65 °C |
| Tank capacity | 8 l |
| Rinse water consumption/Rack P1/P2 | 2,5 l |
|  |  |
| **Values of connection** |  |
| Heating Booster/Tank | 2,8 kW (400 V: 4,2 kW) / 0,8 kW |
| Total loading | 3,2 kW (400 V: 5,4 kW) |
| Rated Voltage | 230 V/50Hz/1 (400V/50Hz/3N) |
|  |
| \* To reach set rinse temperatures even with cold water connection, the actual cycle-times extend accordingly. |
| \*\* Theoretical performance |
|  |
|  |
|  |